version4.0
Lines 1: 3 lines of characters identifying the run (max 72 characters/line)
Typical correlations file for axial turbine - no blockage
Kacker-Okapuu


Line 2: Integers for data and correlations
i_loss   i_dev   i_ewb
 2        2       0

Line 3: Loss input data 
n_loss_bladerow   dummy
  1                1

Line 4: Empirical deviation data (i_loss = 2)
i_blrow  i_loss_type   f_loss(1)  f_loss(2)  f_loss(3)  f_loss(4)  f_loss(5)  f_loss(6)
  1       1	            1.0	    1.0         1.0        1.0       1.0         1.0

Line 5: Deviation input data 
n_dev_bladerow    dummy
    1              1

Line 6: Empirical deviation data
i_blrow  i_dev_type   f_dev(1)  f_dev(2)  f_dev(3)  f_dev(4)  f_dev(5)  f_dev(6)
  1       1	            0.0	    0.0       0.0       0.0      0.0       0.0

Line 7: Blockage input data 
n_ewb_sl  n_ewb_qo
1           1

Line 8: Empirical loss data
i_qo  k_ewb   f_ewb    ewb
1       1     0.500     0.00

