;*****************************************************************************
; DSP56K Highlighting Test File
; Comments look like this
;*****************************************************************************
    PAGE    110,60,1,1
    TABS    4
;*****************************************************************************
;   DEFINITIONS & POINTERS
;*****************************************************************************
START       EQU     $000100                 ; program start location
SERIAL      EQU     $2                      ; serial number location

TXD         EQU     $FFFFBC                 ; ESSI0 Transmit Data Register 0
RXD         EQU     $FFFFB8                 ; ESSI0 Receive Data Register
SSISR       EQU     $FFFFB7                 ; ESSI0 Status Register
CRB         EQU     $FFFFB6                 ; ESSI0 Control Register B
CRA         EQU     $FFFFB5                 ; ESSI0 Control Register A
PCRC        EQU     $FFFFBF                 ; Port C (ESSI_0) control register
PCTL        EQU     $FFFFFD                 ; PLL control register
TXREG       EQU     $FFFF89                 ; external TX register
RXREG       EQU     $FFFF8A                 ; external RX register

PDRB        EQU     $FFFFC9                 ; Port B (HOST) GPIO data
PRRB        EQU     $FFFFC8                 ; Port B (HOST) GPIO direction
PCRB        EQU     $FFFFC4                 ; Port B (HOST) control register

PCRE        EQU     $FFFF9F                 ; Port E (SCI) control register
PRRE        EQU     $FFFF9E                 ; Port E (SCI) data direction
PDRE        EQU     $FFFF9D                 ; Port E (SCI) data


