#### 6.5.7.5. CutoffSelectionRule

`class compolyx.CutoffSelectionRule`(graph, obj, parent=None)

Bases: compolyx.selection_rule.ElementSelectionRule

`angle`

  Cut-Off angle

`cutoff_geometry`

  Cut-off Geometry for the Cut-off Rule

`cutoff_rule_type`

  Cutoff rule type, valid values geometry,variable_taper,taper

`direction`

  Direction of the offset and angle interpolation for 'variable_taper'

`distance_type`

  Distance type for offset and angle interpolation for 'variable_taper'

`edge_set`

  Edge Set for cutoff_rule_type=`taper` or variable_taper

`offset`

  Cut-Off offset

`offset_method`

  Method to compute the offset of a ply.

`offset_type`

  Take offset from edge set perpendicular to element reference surface ( out_of_plane ) or in element reference surface ( in_plane )

`origin`

  Origin of the offset and angle interpolation for 'variable_taper' cutoff rules

`ply_cutoff_type`

  Cutoff Types can be: analysis_ply_cutoff,production_ply_cutoff

`ply_tapering`

  Use Ply Tapering Orientation

Release 18.2 - © ANSYS, Inc. All rights reserved.