### 1.5.4. Solid Modeling

Similar to composite shells, composite solids defined using ACP can be imported into Mechanical for analysis by importing the mesh from upstream ACP systems and synthesizing the geometry from the imported meshes. The import of a composite solide from ACP into Mechanical follows the same procedure for shells except that the transfer option Transfer Solid Composite Data must be selected.

Release 18.2 - © ANSYS, Inc. All rights reserved.