### 3.5.2. User-Defined Draping

ACP can also handle user-defined draping results. The draped fiber directions can be imported as a Look-Up Table and used instead of Internal Draping.

Figure : Tabular Values Definition of Draping

The first angle Correction Angle 1 defines the correction of the material reference direction and is also considered in the analysis. The second value Correction Angle 2 can be used to define the correction angle of the material 2 direction for woven materials. In ACP, the second correction is not considered in any evaluation and is just for information or third party products.

Release 18.2 - © ANSYS, Inc. All rights reserved.