### 1.6.5. Example: Kiteboard

The ability to parameterize an ACP composite model is a powerful design tool. Parameter studies can be carried out efficiently in the Workbench environment. This example focuses on the parameter functionality for the layup of a kiteboard. Input and output parameters are defined in both ACP (Pre) and ACP (Post):

- Control over material choice, ply stackup and selection rules.

- Readout of weight, Inverse Reserve Factor and deformations.

Start ANSYS Workbench and restore the kiteboard.wbpz archive.

Release 18.2 - © ANSYS, Inc. All rights reserved.