#### 3.3.1.2. Class40

The Class40 example uses a tapered core. Open the model and check the Modeling Ply `core_bwl` in the Modeling Group `Hull`. In the Thickness tab of the properties dialog a taper angle of 15 degrees is defined for the edge `edgeset.2`. A Section Cut or thickness contour plot illustrates the final result as shown in Figure : Tapered Edge.

Figure : Tapered Edge

Release 18.2 - © ANSYS, Inc. All rights reserved.