#### 3.5.1.3. Draping Direction

After the first point is applied on the mold, the Draping Direction defines along which route the ply is laid into the mold. The draping algorithm first walks along the Draping Direction, then orthogonal and finally proceeds with the 45-degree zones. Figure : Draping Scheme shows the scheme in which the ply is applied.

Release 18.2 - © ANSYS, Inc. All rights reserved.