#### 3.5.1.5. Draping Definition on OSS Level

The draping can be activated in the Draping tab of the Oriented Selection Set Properties dialog.

Figure : Draping Definition in OSS

If draping is activated on the OSS level, draping is evaluated for all plies linked with this OSS. If the Modeling Ply also has an active draping definition, the OSS draping definition is not used.

Release 18.2 - © ANSYS, Inc. All rights reserved.