### 10.13.9. Parts - Solvers (Structured) - Dezone (2D & 3D Lagrange/ALE)

This window lets you dezone a 2D or 3D Lagrange or ALE Part.

Dezoning involves combining a number of cells in a fine grid into single cells of a coarser grid.

I-factor

  The number of cells in the I direction you want to combine into a single cell. This total number of cells in the I direction (IMAX-1) must be exactly divisible by this number.

J-factor

  The number of cells in the J direction you want to combine into a single cell. This total number of cells in the J direction (JMAX-1) must be exactly divisible by this number.

K-factor

  The number of cells in the K direction you want to combine into a single cell. This total number of cells in the K direction (KMAX-1) must be exactly divisible by this number.

Dezone Range

  In these six fields, enter the range over which the dezone should be performed.

Release 18.2 - © ANSYS, Inc. All rights reserved.