### 5.11.13. Rigid EOS

To access local data

    USE matdef
    USE eos_rigid

C_OF_MASS_X | Initial X position of center of mass
C_OF_MASS_Y | Initial Y position of center of mass
C_OF_MASS_Z | Initial Z position of center of mass
RIGID_MASS | Mass of rigid body
RIGID_IXX | Initial moment of inertia about XX
RIGID_IYY | Initial moment of inertia about YY
RIGID_IZZ | Initial moment of inertia about ZZ
RIGID_IXY | Initial moment of inertia about XY
RIGID_IYZ | Initial moment of inertia about YZ
RIGID_IZX | Initial moment of inertia about ZX
IF_RIGID_CONSTRAINT | Rigid body constraint switch
UX_RB | Constrained X-velocity
UY_RB | Constrained Y-velocity
UZ_RB | Constrained Z-velocity
URX_RB | Constrained URX-velocity
URY_RB | Constrained URY-velocity
URZ_RB | Constrained URZ-velocity

Release 18.2 - © ANSYS, Inc. All rights reserved.