### 10.9.6. Parts - Zoning - Hex

Select Node to Edit

  Use the arrow buttons to select each of the 8 nodes in turn.

Coordinates

  The X, Y, and Z coordinates of the node.

Cells in I/J/K direction

  The number of cells (elements) you want to use in the I, J and K directions. The corresponding number of nodes and elements required for your part will be displayed below.

Automatic

  Select this option if you want the internal nodes to be spaced equipotentially.

IJK-Straight

  Select this option if you want the nodes along each I, J and K line to be equally spaced along a straight line.

Geometric Ratios

  Input geometric ratios in the fields provided if you want to grade the zoning instead of generating equally spaced nodes.

Release 18.2 - © ANSYS, Inc. All rights reserved.