## 5.6. JETDEF, Jetting Variables

Module jetdef includes variables associated with the jetting option. (Autodyn-2D only)

          MODULE jetdef
          USE kindef
          IMPLICIT NONE

          SAVE

          INTEGER, PARAMETER :: LIMJET = 100
          INTEGER, PARAMETER :: MAXJVR = 21
          INTEGER (INT4) :: NUMJET, NXTJET, JETSUB, JETRAP
          INTEGER (INT4), DIMENSION(LIMJET), TARGET :: NPJET, JPJET
          REAL (REAL8) :: VSLBAR, PMSLUG, XMOMSL
          REAL (REAL8), DIMENSION(LIMJET), TARGET :: TIMJET, PMJET, XZJET
          REAL (REAL8), DIMENSION(LIMJET), TARGET :: YZJET
          REAL (REAL8), DIMENSION(LIMJET), TARGET :: XJET, YJET, UXJET, UYJET
          REAL (REAL8), DIMENSION(LIMJET), TARGET :: DXJET, DYJET, VLJET
          REAL (REAL8), DIMENSION(LIMJET), TARGET :: THKJET

          END MODULE jetdef

LIMJET | Limit on number of jetting points
NUMJET | Number of jetting points
NXTJET | Next point to jet
JETSUB | Part containing jetting points
JETRAP | Wrapup indicator
NPJET | Array of jetted points
JPJET | Jetting point index
VSLBAR | Mean slug velocity
PMSLUG | Total slug mass
XMOMSL | Total slug momentum
TIMJET | Time of jetting
PMJET | Jet mass
XZJET | Initial X-coordinate
YZJET | Initial Y-coordinate
XJET | X coordinate at jet formation
YJET | Y coordinate at jet formation
UXJET | X component of collapse velocity
UYJET | Y component of collapse velocity
DXJET | DX of segment at jet formation
DYJET | DY of segment at jet formation
VLJET | Initial volume
THKJET | Initial thickness

Release 18.2 - © ANSYS, Inc. All rights reserved.