### 36.3.2. Axes

The axis of rotation for the turbo component is set relative to the Global Coordinate frame (`Coord 0`) by default. You can choose a user-specified coordinate frame from the drop-down list or create a new one by selecting . For details, see Coordinate Frames. For details, see Coordinate Frames in the CFX-Solver Modeling Guide.

#### 36.3.2.1. Coordinate Frame

Choose a Coordinate Frame or click the to create a new coordinate frame. For details, see Coordinate Frames. For details, see Coordinate Frames in the CFX-Solver Modeling Guide.

#### 36.3.2.2. Rotational Axis

Select the rotational axis relative to the chosen coordinate frame.

#### 36.3.2.3. Axis Visibility

Toggle to select the visibility of the axis.

Release 18.2 - © ANSYS, Inc. All rights reserved.