### 8.4.3. Stopping Runs Using External Solver Couplings

If a stop current run command is issued for a run that uses external solver couplings (for example, ANSYS Multi-field), then the overall simulation is terminated. For ANSYS Multi-field couplings, termination occurs at the end of the current Load Step, for details see the Mechanical APDL Coupled-Field Analysis Guide in the Mechanical APDL Coupled-Field Analysis Guide. In particular, steady-state analyses will run until completion, and transient analyses will run until the end of the current timestep.

Release 18.2 - © ANSYS, Inc. All rights reserved.