## 6.7. Creating a New Throughflow Analysis

You can create a Throughflow analysis using either the Create New > Throughflow (BladeGen) command or the Create New > Throughflow (BladeEditor) command in the right-click context menu of the Blade Design cell.

The first of these commands generates a set of systems as shown below.

The Turbo Setup component is populated with the duty point operating conditions from the Vista CCD calculation.

The Blade Design component is populated with the impeller geometry using the current, up-to-date parameters from the Vista CCD calculation.

The Vista TF system is subsequently created from the up-to-date Turbo Setup system and linked to the upstream impeller Blade Design. The Vista TF system is ready to update to calculate the throughflow analysis in the usual way. See Vista TF User's Guide for further details.

The second of these commands provides the equivalent analysis capability using a Geometry (BladeEditor) component in place of the BladeGen system.

Release 18.2 - © ANSYS, Inc. All rights reserved.