### 2.5.3. CFX-4

Imports a CFX-4 grid file. The external import routine is `ImportCFX4`.

Available options are:

`-v` Verbose output. Echo additional data to `stdout` during the import.

`-C` Read coordinates as being in cylindrical coordinates.

`-i` Included interfaces in regions.

`-3` Include USER3D and POROUS regions as 3D regions.

`-c` Import blocked-off conducting solid regions as 3D regions.

`-l` Include blocked-off solid regions as 3D regions.

`-X` Import axisymmetric problem with default values in geometry file.

`-a <`nk`>` Override the number of planes created in the k direction by `nk` (for example, split theta with `nk` planes) for axisymmetric import.

`-A <`theta`>` Create a total sector of ``theta`` degrees for axisymmetric import.

`-S` Rename multiple symmetry planes with the same name to conform to CFX-Solver requirements (that is, must lie in a plane).

Release 18.2 - © ANSYS, Inc. All rights reserved.