## 3.6. Integration with Vista CCD

The Turbo Setup system is integrated with preliminary designs for centrifugal compressors created by Vista CCD in ANSYS Workbench. The settings used to generate a design in Vista CCD may be transferred to a new Turbo Setup system using the context menu command Create New > Turbo Setup from the Blade Design cell of the Vista CCD system. The resulting Turbo Setup system may then be used to generate Throughflow and Turbomachinery Fluid Flow systems in the usual way.

There are additional context menu commands for generating new Throughflow and Turbomachinery Fluid Flow systems from a Vista CCD system that automate the process of generating the required geometry, Turbo Setup system, and analysis components into a single operation. For details, see Context Menu Commands of the Blade Design Cell in the TurboSystem User's Guide.

Release 18.2 - © ANSYS, Inc. All rights reserved.