## 22.1. Inserting a New Transient Blade Row Models Object

Setting up a Transient Blade Row Model in the CFX-Solver Modeling Guide describes a procedure for inserting a Transient Blade Row Model object.

To insert a `Transient Blade Row Models` object:

1. Do one of the following:

   - Right-click `Flow Analysis 1` (or whichever analysis is applicable) in the Outline tree, then select Insert > Transient Blade Models from the shortcut menu.

   - Select `Flow Analysis 1` (or whichever analysis is applicable) in the Outline tree, then select Insert > Transient Blade Row Models from the main menu.

2. Click OK.

Release 18.2 - © ANSYS, Inc. All rights reserved.