### 2.6.3. Heat Transfer

Specify the Heat Transfer as for an inlet boundary condition. This value is only used for the inflow portion of the opening. You can specify either:

- Static Temperature

- Opening Temperature

  The opening temperature is similar to the `Total Temperature`, but the dynamic component is based only on the normal component of velocity.

Release 18.2 - © ANSYS, Inc. All rights reserved.