### 5.9.6. Energy Equation

For multicomponent fluids, the energy equation has an additional term corresponding to enthalpy transport by species velocities. For standard transported components, this velocity is modeled using Fick’s law. For ASM components, this term uses the drift velocity.

The following term is therefore added to the right-hand side of Equation 2–5:

| (5–193)

Release 18.2 - © ANSYS, Inc. All rights reserved.