### 11.2.3. Postprocessing

If a total pressure inlet boundary condition is used (recommended where possible), it will also provide a useful starting point for streamlines that are colored by total pressure during postprocessing. The uniform total pressure distribution means lines will begin with a uniform color. It may be harder to visually resolve these pressure values if an inlet velocity profile is used.

CFD-Post provides a performance macro for liquid pumps and turbines.

Release 18.2 - © ANSYS, Inc. All rights reserved.