### 10.10.3. Looking at the Auxiliary Views

The Auxiliary view can show either the blade to blade geometry or the blade lean angle at a given time.

Make the Auxiliary view visible as follows:

1. Click Show/Hide Auxiliary Pane as required to show the Auxiliary view.

2. Select `Blade1` from the Tree Outline view.

   The Blade to blade view is displayed for `Blade1`.

3. Right-click inside the Blade to blade view and select Blade Lean Angle.

   The Lean Angle view is displayed for `Blade1`.

The Blade to blade and Lean Angle views are updated if changes are made in the Angle or Thickness views, after you click Generate .

Note: You can view the blade to blade and blade lean angle auxiliary views for the splitter blade in the same way.

Release 18.2 - © ANSYS, Inc. All rights reserved.