### 1.4.2. Defining the Physics of the Model

This interactive process is the second pre-processing stage and is used to create input required by the Solver. The mesh files are loaded into the physics preprocessor, CFX-Pre.

The physical models that are to be included in the simulation are selected. Fluid properties and boundary conditions are specified.

Release 18.2 - © ANSYS, Inc. All rights reserved.