## 3.2. Files Generated by the CFX-Solver

The CFX-Solver typically generates two files for each run: the CFX-Solver Output file and the CFX-Solver Results file. These are discussed in the following sections:

- CFX-Solver Output File

- CFX-Solver Output File (Transient Runs)

- CFX-Solver Output File (Interpolation Runs)

- CFX-Solver Output File (Parallel Runs)

- CFX-Solver Output File (Mesh Adaption Runs)

- CFX-Solver Output File (Remeshing Runs)

- CFX-Solver Output File (Conjugate Heat Transfer Runs)

- CFX-Solver Output File (GGI Runs)

- CFX-Solver Output File (Combustion Runs)

- CFX-Solver Output File (Particle Runs)

- CFX-Solver Output File (ANSYS Multi-field Runs)

- CFX-Solver Output File (Radiation Runs)

- CFX-Solver Output File (Rigid Body Runs)

- CFX-Solver Results File

Additional files are generated for the run as follows:

- For runs that involve the use of the Discrete Transfer or Monte Carlo radiation models, an additional file containing radiation data can also be generated. See CFX Radiation File.

- For parallel runs of the CFX-Solver, an additional CFX partition file can also be generated. See CFX Partition File.

- For ANSYS Multi-field runs, additional files are created. See Additional Files for ANSYS Multi-field Runs.

For multi-configuration simulations, the CFX-Solver generates two additional simulation level text output and results files in addition to the output and results files generated per configuration. These files are discussed in the sections:

- CFX Multi-Configuration Output File

- CFX Multi-Configuration Results File

Release 18.2 - © ANSYS, Inc. All rights reserved.