### 8.4.4. Stopping Multi-Configuration Runs

If a stop run command is issued in a workspace for a specific configuration, then only the current CFX-Solver run for that configuration will be terminated; the overall simulation is not. All remaining configurations that are defined for the simulation are subsequently run (unless a stop run command is also issued for them). If a stop run command is issued in the simulation-level workspace, which is labeled according to the name of the multi-configuration CFX-Solver Input file (`*.mdef`), then the overall simulation is terminated. The CFX-Solver run for the configuration currently being executed is terminated as soon as possible, and no additional configurations are executed.

Release 18.2 - © ANSYS, Inc. All rights reserved.