### 6.7.4. General Postprocessing Guidelines

- Animations:

  - Because the resulting animations of transient blade row cases are usually periodic in time, you must take care not to repeat the start/end point of the period when these are identical. The animation panel has an advanced option to avoid this (the option is named Don't Encode Last MPEG frame), and you should select this option when working with a transient blade row animation.

Release 18.2 - © ANSYS, Inc. All rights reserved.