### 4.1.5. Output from the Performance Map System

As you enter data into the Operating Conditions tab, design points are automatically generated for each participating system:

- One design point at the rotational speed and mass flow rate specified for the base duty operating point, and

- One design point for each mass flow rate of each speedline, using the specified rotational speed for the applicable speedline.

Note: The set of design points generated by the Performance Map system is a subset of the available design points in the parameter manager. Consequently any design points that you create or duplicate using the parameter manager will not appear in the Performance Map system and will not be displayed in the resulting performance map.

Release 18.2 - © ANSYS, Inc. All rights reserved.