### 7.18.1. Interface Compression Level

This controls the volume fraction advection scheme details for free surface flows, which in turn controls the interface sharpness. Allowable values are:

Setting | Value
--- | ---
0 | No special compression — The advection scheme is the same as the global advection scheme setting.
1 | Intermediate compression
2 | Aggressive compression — This is the default.

Release 18.2 - © ANSYS, Inc. All rights reserved.