### 7.11.1. Value

User-defined laminar burning velocity, . It is recommended that you account for dependency on the fuel/oxidizer ratio by making the expression depend on the equivalence ratio or the mixture fraction. Properties of the unburnt mixture (temperature, density, specific heat capacity, thermal conductivity) may be used in the expression in order to account for preheating or mixture dependency.

Release 18.2 - © ANSYS, Inc. All rights reserved.