## 3.4. Creating a New Throughflow System

You can create a Vista TF system, with all the properties appropriately set, using the Create New > Throughflow command in the right-click context menu of the Turbo Setup system’s Turbo Setup cell. The only properties of the Vista TF system’s Setup cell that are not set from the Turbo Setup system are the machine type and the number of blade rows. If the geometry is provided from an upstream blade design, either from BladeGen (a BladeGen system’s Blade Design cell) or BladeEditor (a Geometry system’s Geometry cell), then the machine type and the number of blade rows will be taken from the upstream geometry and will no longer appear in the Properties view. If the geometry is instead provided by an imported geometry file then you must manually specify the machine type and the number of blade rows.

Release 18.2 - © ANSYS, Inc. All rights reserved.