## 6.5. Context Menu Commands of the Blade Design Cell

You can access a context menu for the Blade Design cell in the Vista CCD component system by right-clicking the cell. Most of the commands that are available are standard, and are described in Cells in Workbench. The context menu commands that are specific to the Blade Design cell are described in Table 6.3: Context Menu Commands Specific to the Vista CCD Blade Design Cell.

Table 6.3: Context Menu Commands Specific to the Vista CCD Blade Design Cell

Command | Description
--- | ---
Edit | This command opens the Vista Centrifugal Compressor Design dialog box.
Import BladeGen File | This command first prompts you to select a BladeGen file, then imports the Vista CCD settings from the selected file into the cell properties. The BladeGen file is required to have been written by an older version of BladeGen that included Vista CCD; such an older version of BladeGen wrote Vista CCD settings into the BladeGen file. By contrast, a BladeGen file produced by the Create New > BladeGen command does not contain the Vista CCD data required for the Import BladeGen File command.
Create New > BladeGen | This command creates a BladeGen system that contains a 3D model based on the 1D model in the Vista CCD system. For details, see Launching a New BladeGen Model.
Create New > Geometry | This command creates a Geometry system that contains a 3D model based on the 1D model in the Vista CCD system. For details, see Launching a New BladeEditor Model.
Create New > Turbo Setup | This command creates and populates a Turbo Setup system which can be used to drive either Throughflow or Turbomachinery Fluid Flow analysis systems. For details of the Turbo Setup system, see Turbo Setup in the TurboSystem User's Guide.
Create New > Throughflow (BladeGen) | This command creates and populates Turbo Setup, BladeGen and Vista TF systems ready to perform a throughflow study using Vista TF. For details, see Creating a New Throughflow Analysis.
Create New > Throughflow (BladeEditor) | This command creates and populates Turbo Setup, Geometry (BladeEditor) and Vista TF systems ready to perform a throughflow study using Vista TF. For details, see Creating a New Throughflow Analysis.
Create New > Turbomachinery Fluid Flow (BladeGen) | This command creates and populates Turbo Setup, BladeGen and Turbomachinery Fluid Flow systems ready to perform a CFD study using CFX. For details, see Creating a New Turbomachinery Fluid Flow Analysis.
Create New > Turbomachinery Fluid Flow (BladeEditor) | This command creates and populates Turbo Setup, Geometry (BladeEditor) and Turbomachinery Fluid Flow systems ready to perform a CFD study using CFX. For details, see Creating a New Turbomachinery Fluid Flow Analysis.

Release 18.2 - © ANSYS, Inc. All rights reserved.