### 18.11.2. Supported Independent Thermodynamic Input Properties

The following input properties are currently supported with `USER_STATEPT`:

- Temperature

- Absolute Pressure

- Absolute Pressure and Temperature

- Absolute Pressure and Enthalpy

- Absolute Pressure and Entropy

- Pressure

- Pressure and Temperature

- Pressure and Enthalpy

- Pressure and Entropy

- Mixture Composition (if the material is a variable composition mixture)

The format of the input arguments is an array of property names. The names must be set to the valid short or long names.

Release 18.2 - © ANSYS, Inc. All rights reserved.