## 9.16. Phasic Combustion

Combustion within different phases can be set up using different models with different phases. Refer to the relevant modeling doc for each type of combustion model for advice.

There is no mass transfer between phases for this release of CFX when setting up the default combustion models. You may set this up using interphase mass transfer, but the rates should be sufficiently small that there is no significant mass source.

Release 18.2 - © ANSYS, Inc. All rights reserved.