### 6.8.5. Wall Film Thickness

The wall film thickness on a given (control volume) wall face is computed from the volume fraction, , of all wall particles in a control volume, times the ‘control volume’ volume, , divided by the local control volume face area, :

| (6–198)

The generalization to control volume sectors or element faces is straightforward.

Release 18.2 - © ANSYS, Inc. All rights reserved.