### 3.2.4. CFX-Solver Output File (Interpolation Runs)

This section outlines the additional information that is written to the CFX-Solver Output file for CFX-Solver jobs that require interpolation.

     ======================================================================
                     Interpolating Onto Domain "Bottom Box"
     ======================================================================

     Total Number of Nodes in the Target Domain              =          343
     Bounding Box Volume of the Target Mesh                  =  2.70000E+01

     Checking all source domains from the source file:
       Target mesh is different from domain "Top Box".

     Searching for Candidate Source Domains:

     Warning: The target mesh does not intersect with any source meshes
              that have the same domain type and motion.
              Skip the interpolation.

     ======================================================================
                      Interpolating Onto Domain "Top Box"
     ======================================================================

     Total Number of Nodes in the Target Domain              =          343
     Bounding Box Volume of the Target Mesh                  =  2.70000E+01

     Checking all source domains from the source file:
       Target mesh is the same as domain "Top Box".

     Start direct copying of variables from domain "Top Box".

     +--------------------------------------------------------------------+
     |                     Variable Range Information                     |
     +--------------------------------------------------------------------+
     +--------------------------------------------------------------------+
     |      Variable Name                         |    min    |    max    |
     +--------------------------------------------------------------------+
     | Thermal Conductivity                       |  2.61E-02 |  2.61E-02 |
     | Courant Number                             |  9.86E-02 |  4.52E+00 |
     | Density                                    |  1.18E+00 |  1.18E+00 |
     | Static Entropy                             |  0.00E+00 |  0.00E+00 |
     | Pressure                                   |  1.59E+01 |  6.01E+01 |
     | Specific Heat Capacity at Constant Pressure|  1.00E+03 |  1.00E+03 |
     | Specific Heat Capacity at Constant Volume  |  1.00E+03 |  1.00E+03 |
     | Temperature                                |  2.98E+02 |  2.98E+02 |
     | Velocity                                   |  2.02E-01 |  8.09E+00 |
     | Dynamic Viscosity                          |  1.83E-05 |  1.83E-05 |
     +--------------------------------------------------------------------+

Release 18.2 - © ANSYS, Inc. All rights reserved.