## 12.7. Scale-Resolving Simulations References

###

[1] Boris, J. P., Grinstein, F. F., Oran, E. S., and Kolbe, R. S. “New insights into Large Eddy Simulation”. Fluid Dynamic Research. Vol. 10. 199-228. 1992.

[2] Cokljat D., Caradi D., Link G., Lechner R., and Menter F.R. “Embedded LES Methodology for General-Purpose CFD Solvers”. 22-24 June 2009. Proc. Turbulent Shear Flow Phenomena, 6th Int. Symp. Turbulence and Shear Flow Phenomena. Seoul, Korea. . 1191-1196.

[3] Comte-Bellot, G., and Corrsin, S. “Simple Eulerian time correlation of full- and narrow-band velocity signals in grid-generated, “isotropic” turbulence”. Journal of Fluid Mechanics. Vol. 48, Part 2. 273-337. 1971.

[4] Davidson, L. “Evaluation of the SAS-SST Model “Channel Flow, Asymmetric Diffuser and Axi-Symmetric Hill”. Proceedings European Conference on Computational Fluid Dynamics . ECCOMAS CFD. . 2006.

[5] Durbin, P., and Pettersson Reif, B.A. Statistical theory of turbulent flows. John Wiley and Sons, Ltd. UK. 2003.

[6] Egorov Y., Menter F.R., and Cokljat D. “Scale-Adaptive Simulation Method for Unsteady Flow Predictions. Part 2: Application to Aerodynamic Flow”. Flow Turbulence and Combustion. Vol. 85, No. 1. 139-165. 2010.

[7] Fröhlich J., Mellen C.P., Rodi W., Temmerman L., and Leschziner M. “Highly resolved large-eddy simulation of separated flow in a channel with streamwise periodic constrictions”. Journal of Fluid Mechanics. Vol. 526. 19–66. 2005.

[8] Fröhlich J., and von Terzi, D. “Hybrid LES/RANS methods for simulation of turbulent flows”. Progress in Aerospace Sciences. Vol. 44, Issue 5. 349-377. 2008.

[9] Girimaji, S. S. “Partially-Averaged Navier-Stokes Method: A RANS to DNS Bridging Method”. 2004.

[10] Girimaji, S., and Abdul-Hamid, K.S. “Partially-averaged Navier-Stokes model for turbulence: implementation and validation”. AIAA Aerospace Sciences Meeting and Exhibit. Reno, Nevada. . 2005-0502. 2005.

[11] Gritskevich, M.S. Garbaruk, A.V., Schütze, J., and Menter F.R. “Sensitization of DDES and IDDES Formulations to the Shear-Stress Transport Model”. Flow Turbulence and Combustion. 2012.

[12] Geurts, B. J.. Elements of direct and large-eddy simulation. Edwards Inc. Philadelphia, USA. 2004.

[13] Hanjalic, K., and Launder, B. Modelling Turbulence in Engineering and the Environment. Cambridge University Press. Cambridge, UK. 2011.

[14] Jasak H., Weller H.G., and Gosman A.D. “High Resolution Differencing Scheme for Arbitrarily Unstructured Meshes”. International Journal for Numerical Methods in Fluids. Vol. 31. 431-449. 1999.

[15] Mathey, F., Cokljat, D., Bertoglio, J.P., and Sergent, E. “Specification of LES Inlet Boundary Condition Using Vortex Method. 4th International Symposium on Turbulence, Heat and Mass Transfer. Antalya, Turkey. . 2003.

[16] Menter, F. R. “Two-equation eddy-viscosity turbulence models for engineering applications”. AIAA Journal. Vol. 32, No. 8. 1598–1605. 1994.

[17] Menter F.R., Garbaruk A., and Smirnov P. “Scale adaptive simulation with artificial forcing”. Proc. 3rd Symposium on Hybrid RANS-LES Methods . . 2009.

[18] Menter, F.R., and Egorov, Y. “Scale-Adaptive Simulation Method for Unsteady Flow Predictions. Part 1: Theory and Model Description”. Flow, Turbulence and Combustion . Vol. 85, No. 1. 113––138. 2010.

[19] Menter, F.R., and Kuntz, M. “Adaptation of Eddy-Viscosity Turbulence Models to Unsteady Separated Flow Behind Vehicles”. Proc. Conf. The Aerodynamics of Heavy Vehicles: Trucks, Busses and Trains. Asilomar, California. Springer . . 2002.

[20] Michelassi V., Wissink, J. G., and Rodi W. “Direct numerical simulation, large eddy simulation and unsteady Reynolds-averaged Navier-Stokes simulations of periodic unsteady flow in a low-pressure turbine cascade: A comparison”. Journal of Power and Engineering . Vol 217, Number 4. 403––411. 2003.

[21] Morris S. C. and Foss J. F.. “Turbulent boundary layer to single-stream shear layer: the transition region”. Journal of Fluid Mechanics Fluid Mech.. Vol 494. 187–221. 2003.

[22] Nicoud, F., and Ducros, F. “Subgrid-scale stress modelling based on the square of the velocity gradient tensor”. Flow, Turbulence and Combustion . Vol. 62. 183––200. 1999.

[23] Reichardt, H. “Vollstandige Darstellung der turbulenten Geschwindigkeitsverteilung in glatten Leitungen”. Zeitschrift fur Angewandte Mathematik und Mechanik . Vol. 31. 208––219. 1951.

[24] Rotta, J.C. “Turbulente Strömumgen”. BG Teubner Stuttgart. 1972.

[25] Sagaut, P., Deck, S., and Terracol, M. Multiscale and multiresolution approaches in turbulence. Imperial College Press. London. 2006.

[26] Schildmacher, K.-U., Koch, R., Wittig, S., Krebs, W., and Hoffmann, S. “Experimental investigations of the temporal air-fuel mixing fluctuations and cold flow instabilities of a premixing gas turbine burner”. ASME Paper 2000-GT-0084. 2000.

[27] Shur, M.L., Spalart, P.R., Strelets, M.K., and Travin, A.K. “A hybrid RANS-LES approach with delayed-DES and wall-modeled LES capabilities”. International Journal of Heat and Fluid Flow . Vol. 29. 1638-1649. 2008.

[28] Sjunnesson, A., Henriksson, R., and Lofstrom, C. “CARS measurements and Visualization of Reacting Flows in Bluff Body Stabilized Flame”. AIAA Paper 1992–3650. 1992.

[29] Smagorinsky, J. “General Circulation Experiments with the Primitive Equations”. Monthly Weather Review. Vol. 91. 99–––165. 1963.

[30] Spalart, P.R., Jou, W., Strelets, M., and Allmaras, S. “Comments on the feasibility of LES for wings, and on a hybrid RANS/LES approach”. Advances in DNS/LES. 1st AFOSR Int. Conf. on DNS/LES. . 1997.

[31] Spalart, P. R. “Strategies for turbulence modelling and simulations”. International Journal of Heat and Fluid Flow. Vol. 21. 2. 2000.

[32] Spalart, P., Deck, S., Shur, M., Squires, K., Strelets, M., and Travin, A. “A New Version of Detached Eddy Simulation, Resistant to Ambiguous Grid Densities”. Journal of Theoretical and Computational Fluid Dynamics. Vol. 20. 181––195. 2006.

[33] Strelets, M. “Detached Eddy Simulation of massively separated flows”. AIAA Paper 2001-879. 2001.

[34] Travin, A., Sur M., Strelets, M., and Spalart P. “Physical and numerical upgrades in the detached eddy simulation of complex turbulent flows”, In Advances in LES of complex flows””. eds. R. Friedrich, W. Rodi . Kluwer Acad. New York. 239-254. 2000.

[35] Vogel, J.C., and Eaton, J.K. “Combined heat transfer and fluid dynamic measurements downstream of a backward-facing step”. Journal of Heat and Mass Transfer. Vol. 107. 922––929. 1985.

[36] Wagner, C., Hüttl, T., and Sagaut, P. “Large-eddy simulation for acoustics”. Cambridge University Press. 2007.

[37] Westin, J., Alavyoon F., Andersson, L. Veber, P., Henriksson, M., and Andersson, C. “Experiments and Unsteady CFD-Calculations of Thermal Mixing in a T-Junction” . OECD/NEA/IAEA Workshop on the Benchmarking of CFD Codes for Application to Nuclear Reactor Safety (CFD4NRS). Munich, Germany. . 1–15. 2006.

[38] Widenhorn, A., Noll, B., and Aigner, M. “Numerical Study of a Non-Reacting Turbulent Flow in a Turbine Model Combustor”. AIAA Paper 2009-647, Orlando Florida . 2009.

[39] Wilcox, D.C. “Turbulence Modeling for CFD”. DCW Industries Inc. 3rd Edition. 2006.

Release 18.2 - © ANSYS, Inc. All rights reserved.