### 10.10.6. Summary

This tutorial has demonstrated how to launch a BladeEditor model using data from a Vista CCD system, make a few modifications to the blade, and export the geometry for use in ANSYS TurboGrid or ANSYS Meshing. For more information on manually modifying the blade in BladeEditor, see Tutorial 1: Blade Editing With Emphasis On Sketches, Layers, and Blade Comparison.

Release 18.2 - © ANSYS, Inc. All rights reserved.