### 2.5.4. CFX-5.1

Imports a CFX-5.1 results file. The external import routine is `ImportCFX5`.

Available options are:

`-v` Verbose output. Echo additional data to `stdout` during the import.

`-f` Input file is formatted.

`-u` Input file is unformatted (Fortran).

`-M <`machine type`>` Set the machine type in the case of a binary or unformatted file so that data conversion may be done if needed. The default file format is 32-bit IEEE (Iris, Sun, HP, IBM). The currently recognized machine types are:

- IEEE - generic 32-bit IEEE machine.

- BSIEEE - generic 32-bit byteswapped IEEE machine.

- IBM - IBM 32-bit IEEE.

- IRIS - Iris 32-bit IEEE.

- HP - HP 32-bit IEEE.

- SUN - Sun 32-bit IEEE.

- ALPHA - Compaq Tru64 UNIX Alpha 64-bit byte-swapped IEEE.

- DOS - DOS 16-bit byte-swapped IEEE.

- Compaq Tru64 UNIX - Compaq Tru64 UNIX 32-bit byte-swapped IEEE.

- CRAY - Cray 64-bit format.

- CONVEX - native Convex floating point format.

- Windows - 32-bit Windows.

The argument machine type is case insensitive, and only the first 2 characters are needed (any others are ignored).

`-M` <`machine type`> Set the machine type in the case of a binary or unformatted file so that data conversion may be done if needed. The default file format is 32-bit IEEE (Iris, Sun, HP, IBM). The currently recognized machine types are:

- IEEE - generic 32-bit IEEE machine.

- BSIEEE - generic 32-bit byteswapped IEEE machine.

- IBM - IBM 32-bit IEEE.

- IRIS - Iris 32-bit IEEE.

- HP - HP 32-bit IEEE.

- SUN - Sun 32-bit IEEE.

- ALPHA - Compaq Tru64 UNIX Alpha 64-bit byte-swapped IEEE.

- DOS - DOS 16-bit byte-swapped IEEE.

- Compaq Tru64 UNIX - Compaq Tru64 UNIX 32-bit byte-swapped IEEE.

- CRAY - Cray 64-bit format.

- CONVEX - native Convex floating point format.

- Windows - 32-bit Windows.

The argument machine type is case-insensitive, and only the first two characters are needed (any others are ignored).

Release 18.2 - © ANSYS, Inc. All rights reserved.