### 10.9.2. Editing the Main Blades and Splitter Blades in BladeEditor

Nine blades and nine splitter blades are displayed.

Now that the geometry has been loaded in BladeEditor, you can modify it. Instructions for doing this are provided in the following sections:

- Modifying the Shroud
- Using Blade Comparison Mode While Updating a Control Point on the Shroud
- Changing the Number of Blades
- Changing the Leading Edge
- Adding Camberline/Thickness Definitions on New Layers

#### 10.9.2.1. Modifying the Shroud

In this section, you will change the shroud in various places. Some of these changes will affect the geometries of the main blade and splitter blade.

Modify the meridional sketch at the shroud as follows:

1. In the Tree Outline view, right-click `Blade1` and select Suppress & All Below.

   This is done so that sketches can be seen clearly without the geometry obstructing your view.

   Alternatively to suppressing the blade, you can click Display Model to toggle the visibility of the blade.

2. Hide the Angle and Thickness views by clicking the Show/Hide Angle Pane and Show/Hide Thickness Pane toolbar icons respectively.

3. Select the Sketching tab at the bottom of the Tree Outline view to switch to the Sketching Toolboxes.

4. Click Look At Face/Plane/Sketch and zoom in as appropriate.

   You should see the following sketch in the graphics view:

5. Select TipRadius.

6. In the details view for TipRadius, change Value to `6 cm`.

7. Select InletHeight.

8. In the details view for InletHeight, change Reference Only? to `Yes`.

   InletHeight no longer governs the control point at the blade leading edge on the shroud.

9. In the Modify toolbox, select Drag.

10. Using the mouse, drag the control point at the blade leading edge on the shroud downward and rightward a short distance.

11. Click Generate .

    The upstream portion of the shroud curve, as well as the curves on the other layers, are modified as a result.

12. Select InletHeight.

13. In the details view for InletHeight, change Reference Only? to `No`.

    InletHeight now governs the control point at the blade leading edge on the shroud.

    Note: Note that you could have caused the same modification by leaving InletHeight as a dimension (Reference Only? set to `No`) and changing its value in the details view.

    Changing a key dimension, such as InletHeight, usually causes multiple control points to move. This technique enables you to make large changes to the geometry quickly.

14. Select the Modeling tab.

15. In the Tree Outline view, right-click `Blade1` and select Unsuppress & All Below.

#### 10.9.2.2. Using Blade Comparison Mode While Updating a Control Point on the Shroud

Blade Comparison mode enables you to create a snapshot of the blade. After you create the snapshot, you can make changes to the blade and then compare the current version of the blade to the snapshot.

In this section, you will:

- Take a snapshot of the blade

- Modify the blade angle

- Modify a control point on the shroud

- View the changes you have made

Start Blade Comparison mode.

1. Click Create snapshot .

   A snapshot of the blade in its current state is now stored in BladeEditor.

   Note that BladeEditor can only create a snapshot when the FlowPath, Blade, and Splitter features have been successfully generated.

2. Click Display Model to hide the geometry.

   This is done so that the modifications made to the blade can be seen clearly.

3. Click Comparison On/Off to toggle the visibility of the snapshot.

Modify the blade angle.

1. In the Tree Outline, select `Blade1` > `Blade1_Camberline1`

2. In the Angle view, drag a control point to change the shape of the curve.

   Note that Blade Comparison mode shows you the shape of the curve from the snapshot as well as the present shape of the curve.

Modify a shroud control point as follows:

1. In the Modify toolbox, select Drag.

2. Using the mouse, drag a point on the shroud a short distance.

Note: Instead of dragging the point, you can cause the same modification by making the point a dimension (Reference Only? set to `No`) and changing its value in the details view.

Click Generate to compare the snapshot of the geometry to the present geometry in the 3D viewer.

After the geometry has been generated, you are able to view the differences between the snapshot (shown in pink) and the present geometry. Note that you may have to rotate the geometry and zoom in to see the differences in the geometry.

Click Comparison On/Off to turn off Blade Comparison mode.

Note: To control the snapshot display settings in Blade Comparison mode, click Comparison display option .

#### 10.9.2.3. Changing the Number of Blades

Generate and view the blade row, then reduce the number of blade sets to seven.

1. On the Modeling tab, select `Blade1`.

2. In the Details view for `Blade1`, change FD1, Number of Blade Sets to `7`.

3. Click Generate .

There are now seven main blades and seven splitter blades.

#### 10.9.2.4. Changing the Leading Edge

Adjust the shape of the leading edge of the main blade.

1. In the Details view for `Blade1`, ensure that Leading Edge Details > Type is set to `Ellipse`.

2. Set FD2, Ellipse Ratio at Hub to `1.5`.

3. Set FD3, Ellipse Ratio at Shroud to `1.0`.

4. Click Generate .

Note: You can adjust the leading edge of the splitter blade in the same way.

#### 10.9.2.5. Adding Camberline/Thickness Definitions on New Layers

There is currently a layer at the hub and a layer at the shroud. You can confirm this by clicking `Blade1` in the Tree Outline view and looking at the Camberline/Thickness Definitions property group in the details view.

In this section you will:

- Add a new layer at a constant span fraction value, and use it to add a new camberline/thickness definition subfeature to the main blade and also the splitter blade

- Add a user-defined layer (which involves using a sketch to define the layer) and use it to add a new camberline/thickness definition subfeature to the main blade

- Specify that the thickness distribution on the user-defined layer should be interpolated from the surrounding layers.

Insert a new layer and camberline/thickness definition and interpolate it from the existing layers:

1. In the Tree Outline view, select `FlowPath1`.

   The Details view for `FlowPath1` is displayed.

2. Right-click Layer Details: 2 and select Insert Layer Above.

3. Set Span Fraction 2 to `0.2`.

4. Click Generate .

   The new layer is now ready to be used by any of the blades.

5. In the Tree Outline view, select `Blade1`.

   Note that the tree shows six camberline sub-features under `Blade1`. Although you have added a layer to the flowpath used by the blade, the layer is not initially being used to define a camberline/thickness definition.

6. In the details view for `Blade1`, under Camberline/Thickness Definitions, set Layer 2 to `Yes`.

   This causes a camberline/thickness definition to be created on that layer, as can be confirmed in the tree view, which now shows seven camberline sub-features under `Blade1`.

7. In the details view for `Splitter1`, under Camberline/Thickness Definitions, set Layer 2 to `Yes`.

   This causes a camberline/thickness definition to be created on that layer, as can be confirmed in the tree view, which now shows seven camberline sub-features under `Splitter1`.

8. Click Generate .

Create a sketch to be used in the definition of a user-defined layer:

1. In the Tree Outline view, right-click `Blade1` and select Suppress & All Below.

   This is done so that sketches can be seen clearly without the geometry obstructing your view.

2. Select `MerPlane1` in the Tree Outline view.

3. Click New Sketch .

   A new sketch, `Sketch11`, appears in the Tree Outline view under `MerPlane1`.

4. Ensure that `Sketch11` is selected in the Tree Outline view.

5. Select the Sketching tab at the bottom of the Tree Outline view to switch to the Sketching Toolboxes.

6. Click Look At Face/Plane/Sketch and zoom in as appropriate.

7. Draw an open-ended curve (for example, a line, polyline, spline, or combination thereof) that passes through the blade passage from inlet to outlet, between the previously-added layer and the shroud, without crossing any existing layers.

   If you use more than one curve to produce a chain of curves, test that the chain is unbroken.

Next, use the sketch to create a user-defined layer:

1. On the Modeling tab, right-click `FlowPath1` and select Edit Selections.

2. Click `Sketch11` in the tree view, then, in the details view, click the field beside Sketches for Defined Layer, then click Apply.

3. Click Generate .

   A new layer appears in the Layer Details portion of the details view.

   The span fraction value is an average of the span value over the sketch used to define the layer.

Next, make a camberline/thickness definition for `Blade1` using the user-defined layer:

1. In the Tree Outline view, select `Blade1`.

   Note that the tree shows seven camberline sub-features under `Blade1`. Although you have added a layer to the flowpath used by the blade, the layer is not initially being used to define a camberline/thickness definition.

2. In the details view for `Blade1`, under Camberline/Thickness Definitions, set the layer you previously created to `Yes`.

   This causes a camberline/thickness definition to be created on that layer, as can be confirmed in the tree view, which now shows eight camberline sub-features under `Blade1`.

Next, make the angle and thickness data on the user-defined layer non-editable, so that it is always interpolated:

1. In the Tree Outline under `Blade1`, select the camberline subfeature that corresponds to the layer that you previously created.

2. In the details view, set Angle Definition and Thickness Definition to `Interpolated`.

   This makes the Angle view and Thickness view read-only. Angle data and thickness data are now interpolated from the adjacent camberline-thickness definitions. The control points disappear from the thickness graph.

3. On the Modeling tab, right-click `Blade1` in the Tree Outline view and select Unsuppress & All Below.

   The blade row should be displayed.

Note: If you wanted to add more user-defined layers, you could add more sketch curves by doing either or both of the following:

- Add more curves to an existing sketch that is already used by the FlowPath feature to define at least one layer.

- Create new sketches, and then add them to the FlowPath feature as sketches to be used for layers (under the Sketches for Defined Layer property).

  Remember that, before you can add sketches to the FlowPath feature, you must right-click the FlowPath feature in the Tree Outline view and select Edit Selections.

Release 18.2 - © ANSYS, Inc. All rights reserved.