B.54. HFSS File (HfssProject)

Engineering Knowledge Manager

Administration Guide | Appendix B. Built-in Types - Reference |

B.53. Group (Group) |  | B.55. Icepak Packed Project (IcepakPackProject)
Prev |  | Next

## B.54. HFSS File (HfssProject)

Base Type: `CAE Model File`

File Extensions: .hfss

Properties: This file can contain multiple "Material" and "Design" models.

A "Material" has the following property:

- Frequency Dependent (frequencyDependent): Whether the material is frequency-dependent.

A "Design" has the following properties:

- Design Type (designType): Type of design (HFSS or HFSS-IE)

- Solution Type (solutionType): Solution type

- Excitation Types (excitationTypes): Types of added excitations

- Optimetric Setups (optimetricSetups): Names of added optimetric setups

- Design Notes (designNotes): Design notes

A "Design" can have multiple "Analysis" models, each of which can have the following properties:

- Frequency (frequency): Solution frequency in GHz

- Minimum Frequency (Eigenmode) (minimumFrequency): Minimum frequency in the case of a design with the solution type of eigenmode.

An "Analysis" can have multiple "Frequency Sweep" models, each of which can have following properties:

- Sweep Type (sweepType): Discrete/Fast/Interpolating

- Sweep Start (sweepStart): Sweep-start frequency in GHz

- Sweep Stop (sweepStop): Sweep-stop frequency in GHz

Contains proprietary and confidential information of ANSYS, Inc. and its subsidiaries and affiliates.

Prev | Up / Contents | Next

Release 18.2 - © ANSYS, Inc. All rights reserved.