13.4.10. Correcting an Invalid Layout

Engineering Knowledge Manager

User's Guide | Chapter 13: Defining Process Templates in EKM Studio | 13.4. Defining Process Templates in EKM Studio |

13.4.9. Opening Process Template Files |  | 13.4.11. Editing Process Attributes
Prev |  | Next

### 13.4.10. Correcting an Invalid Layout

If you have a lifecycle or process template (workflow) from an older version of EKM that has an invalid layout, you can make use of the Automatic Layout feature to correct the layout.

To correct an invalid layout:

1. Open the XML file in a text editor.

2. Find the <layout> description.

       <layout>
         <location nodeName="n4123" x="300" y="65" />
         <location nodeName="n1111" x="20" y="65" />
         <location nodeName="n3_New" x="160" y="30" />
       </layout>

3. Remove the <layout> section from the XML and save the file.

4. Reopen the saved file in EKM Studio. The Automatic Layout feature arranges the nodes/stage positions correctly in a graphical view.

Contains proprietary and confidential information of ANSYS, Inc. and its subsidiaries and affiliates.

Prev | Up / Contents | Next

Release 18.2 - © ANSYS, Inc. All rights reserved.