B.55. Icepak Packed Project (IcepakPackProject)

Engineering Knowledge Manager

Administration Guide | Appendix B. Built-in Types - Reference |

B.54. HFSS File (HfssProject) |  | B.56. Icepak Project Data (IcepakProjectData)
Prev |  | Next

## B.55. Icepak Packed Project (IcepakPackProject)

Base Type: `Icepak Project Data`

File Extensions: .tzr

Properties:

- Flow (flow): Flow solved or not

- Temperature (temperature): Temperature solved or not

- Radiation (radiation): Radiation model used

- Flow Regime (flowRegime): Laminar or turbulent flow

- Turbulence Model (turbulenceModel): Turbulence model used

- Natural Convection (naturalConvection): Natural convection model

- Solar Loading (solarLoading): Off/On

- Altitude (altitude): Off/On

- Species (species): Off/On

- Coupled Solver (coupledSolver): Off/On

- Sequential Solution (sequentialSolution): Off/On

- Parameterization (parameterization): Off/Parametric Trials/Optimization

- Parallel Solution (parallelSolution): Off/On

- Time Variation (timeVariation): Steady or transient calculation

- Version (version): The version of Icepak that generated the file

Contains proprietary and confidential information of ANSYS, Inc. and its subsidiaries and affiliates.

Prev | Up / Contents | Next

Release 18.2 - © ANSYS, Inc. All rights reserved.