#### Incompressible Rotor Report Common Content (Shared by Pump, Fan and Hydraulic Turbine Rotor reports)

COMMAND FILE:
  CFX Post Version = 11.0
END


#### Summary Data Table


!summaryDataTable();


#### Blade Loading Chart


!shortheader1("Blade Loading Charts");

!bladeLoadingChart("Blade Loading", "Pressure", $locSpanLow);
!bladeLoadingChart("Blade Loading", "Pressure", $locSpanMid);
!bladeLoadingChart("Blade Loading", "Pressure", $locSpanHigh);


#### Streamwise Charts


!shortheader1("Streamwise Charts");

!streamwiseChart( "Streamwise Plot of Pt and Ps", 10, "Total Pressure in Stn Frame", "Pt", "mass", "Pressure", "Ps", "area" );
!streamwiseChart( "Streamwise Plot of C", 10, "Velocity in Stn Frame", "C", "area" );
!streamwiseChart( "Streamwise Plot of W", 10, "Velocity", "W", "area" );
!streamwiseChart( "Streamwise Plot of Alpha and Beta", 10, "Velocity Alpha", "Alpha", "area", "Velocity Beta", "Beta", "area" );


#### Spanwise Charts


!shortheader1("Spanwise Charts");

!spanwiseChart( "Spanwise Plot of Alpha and Beta", "at LE", $locStreamLE, 20, "Velocity Alpha", "Alpha", "area", "Velocity Beta", "Beta", "area" );
!spanwiseChart( "Spanwise Plot of Alpha and Beta", "at TE", $locStreamTE, 20, "Velocity Alpha", "Alpha", "area", "Velocity Beta", "Beta", "area" );


#### Blade Geometry Plots


!shortheader1("Blade Geometry Plots");

!bladeGeometryPlots();


#### Blade Mesh Plot


!shortheader1("Blade Mesh Plot");

!bladeMeshPlot( $locSpanMid );


#### Blade to Blade Plots


!shortheader1("Blade to Blade Plots");

!bladetobladeContourPlot( "Total Pressure in Stn Frame", "Pt", $locSpanMid, 20 );
!bladetobladeContourPlot( "Total Pressure", "Ptr", $locSpanMid, 20 );
!bladetobladeContourPlot( "Pressure", "Ps", $locSpanMid, 20 );
!bladetobladeContourPlot( "Velocity", "W", $locSpanMid, 20 );

!bladetobladeVectorPlot( $locSpanLow );
!bladetobladeVectorPlot( $locSpanMid );
!bladetobladeVectorPlot( $locSpanHigh );


#### Meridional Plots


!shortheader1("Meridional Plots");

!meridionalContourPlot("Total Pressure in Stn Frame", "Pt", 20);
!meridionalContourPlot("Total Pressure", "Ptr", 20);
!meridionalContourPlot("Velocity", "W", 20);
!meridionalVectorPlot( "Velocity Meridional", "Cm");


#### Circumferential Plots


!shortheader1("Circumferential Plots");

!circContourPlot( "Total Pressure in Stn Frame", "Pt", $locStreamLE, "Blade LE", 20, -1 );
!circContourPlot( "Total Pressure", "Ptr", $locStreamLE, "Blade LE", 20, -1 );
!circContourPlot( "Velocity", "W", $locStreamLE, "Blade LE", 20, -1 );
!circContourPlot( "Total Pressure in Stn Frame", "Pt", $locStreamTE, "Blade TE", 20, 1 );
!circContourPlot( "Total Pressure", "Ptr", $locStreamTE, "Blade TE", 20, 1 );
!circContourPlot( "Velocity", "W", $locStreamTE, "Blade TE", 20, 1 );


#### 3D Streamline Plots


!shortheader1("Streamline Plot");

!circStreamPlot( $locStreamTE, "Blade TE" );


#### End


# Set view to blade geometry view
>setViewportView cmd=set, view=/VIEW:Blade Geometry Isometric 3D View, viewport=1
>centerview 1

