# This computes U values (based on passage parameterization provided)
# upstream and downstream of a splitter blade leading/trailing edge point
# to provide appropriate geometry sizing around the splitter blade.
ATM GA SPLITTER END PROXIMITY GEOMETRY:
  Source Point =
  Passage Parameterization Source =
  High Blade Curve =
  Low Blade Curve =
  Blade End = LE
  Use Pitch Offset Source Point = false
  Use Pitch Offset High Blade Curve = false
  Use Pitch Offset Low Blade Curve = false
  Main Passage Curve =
  Splitter Low Passage Curve =
  Splitter High Passage Curve = 
END
