10 
 0    0.0 0.0 0.0   node_point { le_passage_low_pnt }   
 1    0.0 0.0 0.0   node_curve { le_passage_focal_crv } 
 2    0.0 0.0 0.0   node_curve { le_passage_focal_crv }  
 3    0.0 0.0 0.0   node_curve { le_passage_focal_crv } 
 4    0.0 0.0 0.0   node_point { le_passage_high_pnt }   
 5    0.0 0.0 0.0   node_point { le2b1_pnt } 
 6    0.0 0.0 0.0   node_curve { le_focal_crv } 
 7    0.0 0.0 0.0   node_curve { le_focal_crv }  
 8    0.0 0.0 0.0   node_curve { le_focal_crv } 
 9    0.0 0.0 0.0   node_point { leb1_p_pnt }
 13 
 0       0       1   edge_curve    { le_passage_focal_crv }
 1       1       2   edge_curve    { le_passage_focal_crv }
 2       2       3   edge_curve    { le_passage_focal_crv }
 3       3       4   edge_curve    { le_passage_focal_crv }
 4       0       5   edge_curve    { high_fullb1_crv }
 5       1       6   
 6       2       7    
 7       3       8    
 8       4       9   edge_curve    { low_fullb1_p_crv } 
 9       5       6   edge_curve    { le_focal_crv } 
10       6       7   edge_curve    { le_focal_crv } 
11       7       8   edge_curve    { le_focal_crv }  
12       8       9   edge_curve    { le_focal_crv }
 4 
 0       4   0    4    9    5  
 1       4   1    6   10    5  
 2       4   2    7   11    6  
 3       4   3    8   12    7  

Attribute: Retained Vertices=6, 8
Attribute: Periodic Sign=0, 1
Attribute: Periodic Start Vertex Centered=7
Attribute: Domain Connection=LE, 1, leb1, le2b1, le focal minus, le focal, leading edgeb1
Attribute: Domain Connection=Local Upstream, le focal
Attribute: Domain Connection=Global Inlet, in ext
Attribute: Projection Object Map=Blade Centric,le_focal_crv,le_focal_minus_crv
# Specify boundary layer edge on both sides of blade.  If it is cutoff at both
# ends, then there are 2 boundary layers.  Otherwise, they will turn out to have the
# same master edge.
# format: edge number, vertex number (of vertex on blade), blade #
Attribute: Edge Distribution Model=Boundary Layer, 9, 5, 1
Attribute: Edge Distribution Model=Boundary Layer, 12, 9, 1

Attribute: Geometry=CreatePoint.ccl, leb1, Create Pitch Offset Geometry=on, Compute Reference Theta=on, Point Type = LE, Create Alternate Geometry = yes, Blade Number = 1
Attribute: Geometry=CreatePoint.ccl, le2b1, Create Pitch Offset Geometry=on, Reference Theta Source=leb1, Point Type = LE2, Create Alternate Geometry = yes, Blade Number = 1
Attribute: Geometry=CreatePoint.ccl, in constant theta, Reference Theta Source=leb1, Point Type = Object and Curve Key, Geometry Object = /GEOMETRY/INLET, Geometry Key = constant theta extended, Set Theta To Reference Theta = on, Create Pitch Offset Geometry=on, Create Alternate Geometry = yes
Attribute: Geometry=CreateCurve.ccl, in ext, Create Pitch Offset Geometry=off, Source Point=in constant theta, Curve Type = Rotation, Geometry Object = /GEOMETRY/INLET, Geometry Key = extended full, Create Alternate Geometry = yes
Attribute: Geometry=CreateBladeCurves.ccl, b1, Create Pitch Offset Geometry=on, Reference Theta Source=leb1, Create Alternate Geometry = yes, Blade Number = 1, Blade Label = b1
Attribute: Geometry=Expose.ccl, low fullb1, Geometry Source = b1, Geometry Reference Name = Low Full
Attribute: Geometry=Expose.ccl, high fullb1, Geometry Source = b1, Geometry Reference Name = High Full
Attribute: Geometry=Expose.ccl, leading edgeb1, Geometry Source = b1, Geometry Reference Name = Leading Edge
Attribute: Geometry=ProjectedPoint.ccl, le focal low, Source Point = le2b1, Use Pitch Offset Source Point = false, Projection Object = high fullb1, Working Space = Transformed
Attribute: Geometry=ProjectedPoint.ccl, le focal high, Source Point = leb1, Use Pitch Offset Source Point = true, Projection Object = low fullb1, Use Pitch Offset Projection Object = true, Working Space = Transformed
Attribute: Geometry=PassageCurve.ccl, le passage focal, Passage Curve Type = LE Pinning Line, Passage Parameterization Source = passageb1, Pinning Line Model = Cutoff
# ================
#   focal curves
# ================
# -- need extra point
Attribute: Geometry=TranslatedPoint.ccl, leb1tra, Source Point=leb1, Pitch Multiple=1
Attribute: Geometry=CurveFromPoints.ccl, le focal, Point List = le2b1$ leb1tra
# -- need extra point
Attribute: Geometry=TranslatedPoint.ccl, le2b1Mtra, Source Point=le2b1, Pitch Multiple=-1
Attribute: Geometry=CurveFromPoints.ccl, le focal minus,  Point List = le2b1Mtra$ leb1

Attribute: Geometry=ComputeDistance.ccl, le blade height, Source Point = leb1, Second Source Point = le2b1, Working Space = Transformed
Attribute: Geometry=ComputeDistance.ccl, le passage height, Source Point = leb1, Use Pitch Offset Source Point = true, Second Source Point = le2b1, Working Space = Transformed
