# Create a point by intersecting a curve with the span surface. The curve can
# be one of the speciofied blade curves (LE, LE2, LEFocal, TE, TE2, TEFocal)
# or it can be specifed by a TG geometry object and curve key (set 'Point Type' to
# 'Object and Curve Key').  Point is initially created in cartesian space and
# maybe converted to transformed space.
ATM GA POINT:
  Point Type =
  Create Pitch Offset Geometry = no
  Create Alternate Geometry = no
  Compute Reference Theta = no
  Blade Number = 1
  Geometry Object =
  Geometry Key =
  Set Theta To Reference Theta = no
  Reference Theta Source =
END