include: herringbone.atf, bladeEnd=te, bladeSide1=low, bladeSide2=high, \
                          bladeSide1PSuffix=_p, bladeSide2PSuffix=, \
                          point1Suffix=2, point2Suffix=, \
                          face0Edge2=4, face0Edge4=5

include: herringboneAttributes.atf, periodicSignVertex=0, \
                                    opening=out, openingU=OUT, openingT=Out, \
                                    bladeEnd=te, bladeEndU=TE, \
                                    position=trailing, positionT=Trailing, \
                                    direction=Down
