-- $Revision: 1.1 $
-----
----- Unix based BATCH terminal in/out template -----
-----
----- Under some versions of AIX on IBM RISC System/6000 machines and Cray X/MP
----- units 5 and 6 are NOT pre-allocated.  In this case, change the
----- definitions to those commented out below.
-----
----- interactive terminal input -----
--tri,10,form,/dev/tty
tri,5,form,
----- interactive terminal output -----
--tro,20,form,/dev/tty
tro,6,form,
----- redirected batch terminal input ------
bti, ,form,*tri
----- redirected batch terminal output ------
bto, ,form,*tro
