# This creates geometry (based on passage parameterization provided)
# to provide appropriate sizing for single herringbone topology.
# 'Herringbone Direction' is used to specify whether the herringbone goes into the
# 'High' or 'Low' corner.
ATM GA SINGLE HERRINGBONE PROXIMITY GEOMETRY:
  Blade End = LE
  Passage Parameterization Source =
  High Curve =
  Low Curve =
  Main Passage Curve =
END
